{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Plan1","Boletim Produção","Boletim Parada"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Plan1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Boletim Produção","index":1,"n_rows":80,"n_cols":42,"rows_kept":80,"cut":false,"hidden":false,"merged":[[3,27,3,28],[3,14,3,17],[3,18,3,19],[3,20,3,21],[3,24,4,24],[3,25,4,25],[3,26,4,26],[2,0,2,11],[2,12,2,17],[2,18,2,21],[2,22,2,23],[2,24,2,26],[3,0,3,1],[3,2,3,5],[3,6,3,8],[3,9,3,11],[3,12,3,13],[0,28,0,31],[1,9,1,10],[1,11,1,12],[1,13,1,14],[1,15,1,16],[1,17,1,18],[1,19,1,20],[1,21,1,22],[1,23,1,24],[1,25,1,26],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,25,0,26],[0,0,1,0],[0,1,1,2],[0,3,1,8],[0,9,0,10],[0,11,0,12],[0,13,0,14]]}
[null,"PAL",null,"BOLETIM DE PRODUÇÃO",null,null,null,null,null,"TURNO",null,"DATA",null,"RESPONSÁVEL",null,"TRS TURNO",null,"NÃO RITMO",null,"INTERRUP.",null,"PREPARAÇÃO",null,"PARADAS",null,"FOLHA Nº"]
[null,null,null,null,null,null,null,null,null,"-",null,null,null,null,null,{"$f":"IF($AH$5=\"\",\"\",100*SUM($M:$M)/$AH$5)","v":40.939507233126832},null,{"$f":"IF($P$2=\"\",\"\",100-$P$2-$T$2-$V$2)","v":11.236311946556903},null,{"$f":"IF($AF$5=\"\",\"\",100*($AF$5/($AD$5-$AE$5)))","v":16.997369532036505},null,{"$f":"IF($AH$5=\"\",\"\",100*($AG$5/($AD$5-$AE$5)))","v":30.826811288279764},null,{"$f":"IF($AE$5=\"\",\"\",IF($AE$5=0,\"\",$AE$5/24))","v":"06:53:34"},null,1]
["CARREGAMENTO DO FORNO",null,null,null,null,null,null,null,null,null,null,null,"PRODUÇÃO LÍQUIDA",null,null,null,null,null,"PERDAS DE PROCESSO",null,null,null,"FORNO",null,"PRODUTIVIDADE (%)"]
["DADOS DE    RASTREAMENTO",null,"DIMENSÕES TUBOS\nLAMINADOS",null,null,null,"DADOS DO MATERIAL",null,null,"DADOS DO BLOCO",null,null,"EMPREGO",null,"REALIZADO",null,null,null,"DEVOLUÇÕES",null,"SUCATAS",null,"HORA",null,"TRS","NÃO    RITMO","PREPARAÇÃO + INTERRUPÇÃO","RITMO TRS [pç/h]",null,"TEMPO TOTAL [h]","PARADAS [h]","INTERRUPÇÕES [h]","PREPARAÇÃO [h]","PEÇAS TRS"]
["ORDEM DE PROCESSO","CARTÃO Nº","DIÂMETRO\nEXTERNO","PAREDE","CMP.QTE LAM3","CMP.  BRUTO FINAL","CORRIDA","AÇO","AQA","DIÂMETRO\nBLOCO ","PESO\nUNITÁRIO","CMP.              BLOCO","PEÇAS","PESO BRUTO","PEÇAS","PESO BRUTO","PEÇAS ACUM","PESO BRUTO ACUM.","QTD","PESO BRUTO","QTD","PESO BRUTO","INÍCIO","TÉRMINO",null,null,null,"%","TOTAL:",{"$f":"IF(AD6=\"\",\"\",SUM(AD6:AD65536))","v":23.999999999999975},{"$f":"IF(AD6=\"\",\"\",SUM(AE6:AE65536))","v":6.8927777777777743},{"$f":"IF(AD6=\"\",\"\",SUM(AF6:AF65536))","v":2.9077777777777749},{"$f":"IF(AD6=\"\",\"\",SUM(AG6:AG65536))","v":5.2736111111110979},{"$f":"IF(AD6=\"\",\"\",SUM(AH6:AH65536))","v":867.13305555555462},"DATA/HORA INÍCIO","DATA/HORA TÉRMINO","Tempo Liquido [min]","Peças Hora Real","Paradas Plano","Interrupção","Preparação","Filtro"]
["LA08550405","582",273.10000000000002,15.11,13.12,12.96,136937,"SAE 4133 NBVTI","TB20","230",1309.8,4.0309999999999997,22,{"$f":"IF(A6=\"\",\"\",M6*K6)","v":28815.599999999999},22,{"$f":"IF(N6=\"\",\"\",IF(AND(T6=\"\",V6=\"\"),N6,IF(T6=\"\",N6-V6,IF(V6=\"\",N6-T6,(N6-T6-V6)))))","v":28815.599999999999},{"$f":"IF(A6=\"\",\"\",O6)","v":22},{"$f":"IF(P6=\"\",\"\",P6)","v":28815.599999999999},0,{"$f":"IF(S6=\"\",\"\",(K6*S6))","v":0},0,{"$f":"IF(U6=\"\",\"\",(K6*U6))","v":0},"00:00:00","00:43:00",{"$f":"IF(M6=\"\",\"\",100*(M6/AC6/(AD6-AE6)))","v":71.251855517070737},{"$f":"IF(AA6=\"\",\"\",100-Y6-AA6)","v":28.748144482929263},{"$f":"IF(M6=\"\",\"\",100*(AF6+AG6)/(AD6-AE6))","v":0},100,55,0.72833333333333306,0.16694444444444401,null,null,{"$f":"IF(AC6=\"\",\"\",AC6*(AD6-AE6))","v":30.876388888888897},"01/03/16 00:00:00","01/03/16 00:43:42",{"$f":"IF(AD6=\"\",\"\",ROUND(60*(AD6-SUM(AE6:AG6)),1))","v":33.700000000000003},{"$f":"IF(AK6=\"\",\"\",M6/AK6*60)","v":39.169139465875361},{"$f":"AE6/24","v":"00:10:01"},{"$f":"AF6/24","v":"00:00:00"},{"$f":"AG6/24","v":"00:00:00"},"00:10:00"]
["LA08551102","583",273.10000000000002,15.11,13.22,13.06,136946,"SAE 4133 NBVTI","TB20","230",1319.5,4.0620000000000003,22,{"$f":"IF(A7=\"\",\"\",M7*K7)","v":29029},22,{"$f":"IF(N7=\"\",\"\",IF(AND(T7=\"\",V7=\"\"),N7,IF(T7=\"\",N7-V7,IF(V7=\"\",N7-T7,(N7-T7-V7)))))","v":29029},{"$f":"IF(A7=\"\",\"\",Q6+O7)","v":44},{"$f":"IF(P7=\"\",\"\",R6+P7)","v":57844.6},0,{"$f":"IF(S7=\"\",\"\",(K7*S7))","v":0},0,{"$f":"IF(U7=\"\",\"\",(K7*U7))","v":0},"00:43:00","01:11:00",{"$f":"IF(M7=\"\",\"\",100*(M7/AC7/(AD7-AE7)))","v":85.257548845470822},{"$f":"IF(AA7=\"\",\"\",100-Y7-AA7)","v":14.742451154529178},{"$f":"IF(M7=\"\",\"\",100*(AF7+AG7)/(AD7-AE7))","v":0},100,55,0.46916666666666601,null,null,null,{"$f":"IF(AC7=\"\",\"\",AC7*(AD7-AE7))","v":25.804166666666632},"01/03/16 00:43:42","01/03/16 01:11:51",{"$f":"IF(AD7=\"\",\"\",ROUND(60*(AD7-SUM(AE7:AG7)),1))","v":28.2},{"$f":"IF(AK7=\"\",\"\",M7/AK7*60)","v":46.808510638297875},{"$f":"AE7/24","v":"00:00:00"},{"$f":"AF7/24","v":"00:00:00"},{"$f":"AG7/24","v":"00:00:00"},"00:00:00"]
["LA08551101","584",273.10000000000002,15.11,13.22,13.06,136945,"SAE 4133 NBVTI","TB20","230",1319.5,4.0620000000000003,2,2639,2,2639,{"$f":"IF(A8=\"\",\"\",Q7+O8)","v":46},{"$f":"IF(P8=\"\",\"\",R7+P8)","v":60483.6},0,0,0,0,"01:11:00","08:00:00",47.430830039523769,52.569169960476231,0,100,55,6.8025000000000002,6.7258333333333304,null,null,4.2166666666668373,"01/03/16 01:11:51","01/03/16 08:00:00",4.5999999999999996,26.086956521739133,"06:43:33","00:00:00","00:00:00","06:43:33"]
["LA08551101","584",273.10000000000002,15.11,13.22,13.06,136945,"SAE 4133 NBVTI","TB20","230",1319.5,4.0620000000000003,19,25070.5,19,25070.5,65,85554.1,0,0,0,0,"08:00:00","08:30:00",68.032623831311028,31.967376168688972,0,100,55,0.507777777777777,null,null,null,27.927777777777735,"01/03/16 08:00:00","01/03/16 08:30:28",30.5,37.377049180327873,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LA08550413","585",273.10000000000002,15.11,13.12,12.96,46973,"SAE 4133 NBVTI","TB20","230",1309,4.0309999999999997,1,1309,1,1309,66,86863.1,0,0,0,0,"08:30:00","08:32:00",71.146245059288688,28.853754940711312,0,100,55,2.5555555555555502E-2,null,null,null,1.4055555555555526,"01/03/16 08:30:28","01/03/16 08:32:00",1.5,40,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LA08550416","586",273.10000000000002,15.11,13.12,12.96,46976,"SAE 4133 NBVTI","TB20","230",1309,4.0309999999999997,1,1309,1,1309,67,88172.1,0,0,0,0,"08:32:00","08:34:00",46.753246753246856,53.246753246753144,0,100,55,3.8888888888888799E-2,null,null,null,2.138888888888884,"01/03/16 08:32:00","01/03/16 08:34:20",2.2999999999999998,26.086956521739133,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LA08550414","587",273.10000000000002,15.11,13.12,12.96,46974,"SAE 4133 NBVTI","TB20","230",1309,4.0309999999999997,1,1309,1,1309,68,89481.1,0,0,0,0,"08:34:00","08:35:00",105.57184750733151,-5.5718475073315119,0,100,55,1.7222222222222201E-2,null,null,null,0.94722222222222108,"01/03/16 08:34:20","01/03/16 08:35:22",1,60,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LA08550415","588",273.10000000000002,15.11,13.12,12.96,46975,"SAE 4133 NBVTI","TB20","230",1309,4.0309999999999997,1,1309,1,1309,69,90790.1,0,0,0,0,"08:35:00","08:38:00",38.730500268961841,61.269499731038159,0,100,55,4.69444444444444E-2,null,null,null,2.5819444444444422,"01/03/16 08:35:22","01/03/16 08:38:11",2.8,21.428571428571431,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LAX0109201","589",273.10000000000002,15.11,13.12,12.99,46970,"SAE 4133 NBVTI","TB20","230",1309,4.04,1,1309,1,1309,70,92099.1,0,0,0,0,"08:38:00","08:38:00",152.21987315010628,-52.219873150106281,0,100,55,1.19444444444444E-2,null,null,null,0.656944444444442,"01/03/16 08:38:11","01/03/16 08:38:54",0.7,85.714285714285722,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LAX0109202","590",273.10000000000002,15.11,13.12,12.99,46969,"SAE 4133 NBVTI","TB20","230",1309,4.04,1,1309,1,1309,71,93408.1,0,0,0,0,"08:38:00","08:41:00",37.402597402597408,62.597402597402592,0,100,55,4.8611111111111098E-2,null,null,null,2.6736111111111103,"01/03/16 08:38:54","01/03/16 08:41:49",2.9,20.689655172413794,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LAX0109203","591",273.10000000000002,15.11,13.12,12.99,46972,"SAE 4133 NBVTI","TB20","230",1309,4.04,1,1309,1,1309,72,94717.1,0,0,0,0,"08:41:00","08:43:00",56.426332288401291,43.573667711598709,0,100,55,3.2222222222222201E-2,null,null,null,1.772222222222221,"01/03/16 08:41:49","01/03/16 08:43:45",1.9,31.578947368421051,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LAX0109204","592",273.10000000000002,15.11,13.12,12.99,46971,"SAE 4133 NBVTI","TB20","230",1309,4.04,1,1309,1,1309,73,96026.1,0,0,0,0,"08:43:00","08:46:00",33.739456419868844,66.260543580131156,0,100,55,5.3888888888888799E-2,null,null,null,2.9638888888888841,"01/03/16 08:43:45","01/03/16 08:46:59",3.2,18.75,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LA08592801","1",273,12.7,13,12.89,136659,"GR B","D024","230",1072.4000000000001,3.2949999999999999,9,9651.6,9,9651.6,82,105677.70000000001,0,0,0,0,"08:46:00","09:06:00",45.646661031276423,26.711749788672865,27.641589180050712,100,60,0.32861111111111102,null,null,9.0833333333333294E-2,19.716666666666661,"01/03/16 08:46:59","01/03/16 09:06:42",14.3,37.76223776223776,"00:00:00","00:00:00","00:05:27","00:05:27"]
["LA08594801","2",273.10000000000002,12.7,13.34,13.18,136670,"GR  B","D024","230",1095.3,3.3690000000000002,8,8762.4,8,8762.4,90,114440.1,0,0,0,0,"09:06:00","09:15:00",90.056285178236735,9.9437148217632654,0,100,60,0.148055555555555,null,null,null,8.8833333333332991,"01/03/16 09:06:42","01/03/16 09:15:35",8.9,53.932584269662918,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LA08551202","3",273.10000000000002,20.239999999999998,13.01,12.89,136944,"SAE 4133 NBVTI","TB20","230",1748.5,5.3819999999999997,18,31473,18,31473,108,145913.1,0,0,0,0,"09:15:00","10:27:00",41.455550437586403,6.1031782588668051,52.441271303546792,100,36,1.20611111111111,null,null,0.63249999999999995,43.419999999999959,"01/03/16 09:15:35","01/03/16 10:27:57",34.4,31.395348837209305,"00:00:00","00:00:00","00:37:57","00:37:57"]
["LA08551201","4",273.10000000000002,20.239999999999998,13.01,12.89,136943,"SAE 4133 NBVTI","TB20","230",1748.5,5.3819999999999997,26,45461,26,45461,134,191374.1,0,0,0,0,"10:27:00","11:24:00",76.80945347119652,13.559822747415,9.6307237813884807,100,36,0.94027777777777699,null,null,9.05555555555555E-2,33.849999999999973,"01/03/16 10:27:57","01/03/16 11:24:22",51,30.588235294117645,"00:00:00","00:00:00","00:05:26","00:05:26"]
["LA08602001","5",273,21.44,9.74,12.8,136926,"GR B","C033","230",1729,5.32,6,10374,5,8645,139,200019.1,0,0,1,1729,"11:24:00","14:02:00",6.3431652394544873,1.7866582091130994,91.870176551432408,100,36,2.6274999999999999,null,2.3272222222222201,8.66666666666666E-2,94.59,"01/03/16 11:24:22","01/03/16 14:02:01",12.8,28.125,"00:00:00","02:19:38","00:05:12","02:24:50"]
["LA08594602","6",273.10000000000002,25.4,12.43,12.32,136926,"GR  B","C033","230",1940.3,5.9660000000000002,4,7761.2,4,7761.2,143,207780.30000000002,0,0,0,0,"14:02:00","14:20:00",36.264732547597568,27.379873073436158,36.355394378966274,100,36,0.30638888888888799,null,null,0.111388888888888,11.029999999999967,"01/03/16 14:02:01","01/03/16 14:20:24",11.7,20.512820512820515,"00:00:00","00:00:00","00:06:41","00:06:41"]
["LA08594601","7",273.10000000000002,25.4,12.43,12.32,136827,"GR  B","C033","230",1940,5.9660000000000002,2,3880,2,3880,145,211660.30000000002,0,0,0,0,"14:20:00","14:23:00",97.560975609756156,2.4390243902438442,0,100,36,5.6944444444444402E-2,null,null,null,2.0499999999999985,"01/03/16 14:20:24","01/03/16 14:23:49",3.4,35.294117647058826,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LA08602401","8",273.10000000000002,31.75,9.85,9.52,136861,"DIN ST 52","C028","230",1803.8,5.548,4,7215.2,4,7215.2,149,218875.50000000003,0,0,0,0,"14:23:00","14:49:00",26.246719160105002,0.459317585301946,73.293963254593052,100,36,0.42333333333333301,null,null,0.31027777777777699,15.239999999999988,"01/03/16 14:23:49","01/03/16 14:49:13",6.8,35.294117647058826,"00:00:00","00:00:00","00:18:37","00:18:37"]
["LA08597501","9",273,36.5,6.9,6.82,136862,"VMEC 134 AP","C030","230",1472.3,4.532,4,5889.2,4,5889.2,153,224764.70000000004,0,0,0,0,"14:49:00","15:19:00",21.845985800109233,38.503549972692639,39.650464227198128,100,36,0.50861111111111101,null,null,0.20166666666666599,18.309999999999995,"01/03/16 14:49:13","01/03/16 15:19:44",18.399999999999999,13.043478260869566,"00:00:00","00:00:00","00:12:06","00:12:06"]
["LA08583201","10",273,36.5,6.9,6.82,136561,"VMEC 134 AP","C030","230",1472,4.532,2,2944,2,2944,155,227708.70000000004,0,0,0,0,"15:19:00","15:23:00",91.324200913242052,8.675799086757948,0,100,36,6.0833333333333302E-2,null,null,null,2.1899999999999991,"01/03/16 15:19:44","01/03/16 15:23:23",3.7,32.432432432432428,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LA08583202","11",273,36.5,6.9,6.82,136862,"VMEC 134 AP","C030","230",1472,4.532,2,2944,2,2944,157,230652.70000000004,0,0,0,0,"15:23:00","15:27:00",91.743119266055118,8.2568807339448824,0,100,36,6.0555555555555501E-2,null,null,null,2.1799999999999979,"01/03/16 15:23:23","01/03/16 15:27:01",3.6,33.333333333333336,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LA08583101","12",259,30,7.89,8.15,136862,"VMEC 134 AP","C030","230",1400.7,4.3079999999999998,6,8404.2000000000007,6,8404.2000000000007,163,239056.90000000005,0,0,0,0,"15:27:00","15:51:00",40.760869565217476,3.5326086956521578,55.706521739130366,100,36,0.40888888888888802,null,null,0.227777777777777,14.719999999999969,"01/03/16 15:27:01","01/03/16 15:51:33",10.9,33.027522935779821,"00:00:00","00:00:00","00:13:40","00:13:40"]
["LA08589801","13",259,30,7.93,8.19,136862,"VMEC 134 AP","C030","230",1407.2,4.3319999999999999,4,5628.8,4,5628.8,167,244685.70000000004,0,0,0,0,"15:51:00","16:00:00",78.895463510848302,21.104536489151698,0,100,36,0.14083333333333301,null,null,null,5.0699999999999878,"01/03/16 15:51:33","01/03/16 16:00:00",8.4,28.571428571428569,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LA08589801","13",259,30,7.93,8.19,136862,"VMEC 134 AP","C030","230",1407.2,4.3319999999999999,2,2814.4,2,2814.4,169,247500.10000000003,0,0,0,0,"16:00:00","16:02:00",131.5789473684211,-31.578947368421098,0,100,36,4.2222222222222203E-2,null,null,null,1.5199999999999994,"01/03/16 16:00:00","01/03/16 16:02:32",2.5,48,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LA08585601","14",259,36.5,6.9,6.82,136862,"VMEC 134 AP","C030","230",1472.3,4.532,4,5889.2,4,5889.2,173,253389.30000000005,0,0,0,0,"16:02:00","16:18:00",41.365046535677365,19.027921406411885,39.60703205791075,100,36,0.26861111111111102,null,null,0.10638888888888801,9.6699999999999964,"01/03/16 16:02:32","01/03/16 16:18:39",9.6999999999999993,24.742268041237114,"00:00:00","00:00:00","00:06:23","00:06:23"]
["LA08594001","15",355.6,9.5,12.13,11.97,136877,"GRADE 290","M068","230",1001,3.08,12,12012,12,12012,185,265401.30000000005,0,0,0,0,"16:18:00","19:34:00",5.6447713998249176,3.3071565770734139,91.048072023101668,100,65,3.2705555555555499,null,null,2.9777777777777699,212.58611111111074,"01/03/16 16:18:39","01/03/16 19:34:53",17.600000000000001,40.909090909090907,"00:00:00","00:00:00","02:58:40","02:58:40"]
["LA08595001","16",355.6,9.52,13.49,13.3,136668,"GR B","D024","230",1114.7,3.431,9,10032.300000000001,9,10032.300000000001,194,275433.60000000003,0,0,0,0,"19:34:00","19:48:00",60.346433227789277,10.597876699571472,29.055690072639251,100,65,0.22944444444444401,null,null,6.6666666666666596E-2,14.913888888888861,"01/03/16 19:34:53","01/03/16 19:48:39",9.8000000000000007,55.102040816326522,"00:00:00","00:00:00","00:04:00","00:04:00"]
["LA08595002","17",355.6,9.52,13.49,13.3,136830,"GR B","D024","230",1114.7,3.431,6,6688.2000000000007,6,6688.2000000000007,200,282121.80000000005,0,0,0,0,"19:48:00","19:56:00",73.682415145830248,26.317584854169752,0,100,65,0.12527777777777699,null,null,null,8.1430555555555042,"01/03/16 19:48:39","01/03/16 19:56:10",7.5,48,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LA08598101","18",355.6,9.5,13.2,13.02,136878,"GRADE 290","M068","230",1088.7,3.351,9,9798.3000000000011,9,9798.3000000000011,209,291920.10000000003,0,0,0,0,"19:56:00","20:08:00",64.819445833750166,35.180554166249834,0,100,65,0.213611111111111,null,null,null,13.884722222222216,"01/03/16 19:56:10","01/03/16 20:08:59",12.8,42.1875,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LA08598102","19",355.6,9.5,13.2,13.02,136878,"GRADE 290","M068","230",1088.5,3.351,2,2177,2,2177,211,294097.10000000003,0,0,0,0,"20:08:00","20:11:00",83.916083916084077,16.083916083915923,0,100,65,3.6666666666666597E-2,null,null,null,2.3833333333333289,"01/03/16 20:08:59","01/03/16 20:11:11",2.2000000000000002,54.545454545454547,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LA08600803","20",355.6,7.9,12.34,12.15,136918,"SAE 41B30H MOD.","U090","230",851.5,2.6179999999999999,16,13624,16,13624,227,307721.10000000003,0,0,0,0,"20:11:00","20:43:00",49.896049896049945,38.045738045737991,12.058212058212062,100,60,0.53444444444444394,null,null,6.4444444444444401E-2,32.066666666666634,"01/03/16 20:11:11","01/03/16 20:43:15",28.2,34.042553191489361,"00:00:00","00:00:00","00:03:52","00:03:52"]
["LA08600804","21",355.6,7.9,12.34,12.15,136918,"SAE 41B30H MOD.","U090","230",851.5,2.6179999999999999,6,5109,6,5109,233,312830.10000000003,0,0,0,0,"20:43:00","20:52:00",63.38028169014116,36.61971830985884,0,100,60,0.15777777777777699,null,null,null,9.4666666666666188,"01/03/16 20:43:15","01/03/16 20:52:43",9.5,37.89473684210526,"00:00:00","00:00:00","00:00:00","00:00:00"]
["LA08600802","22",355.6,7.9,12.34,12.15,136920,"SAE 41B30H MOD.","U090","230",851.5,2.6179999999999999,68,{"$f":"IF(A40=\"\",\"\",M40*K40)","v":57902},65,{"$f":"IF(N40=\"\",\"\",IF(AND(T40=\"\",V40=\"\"),N40,IF(T40=\"\",N40-V40,IF(V40=\"\",N40-T40,(N40-T40-V40)))))","v":55347.5},{"$f":"IF(A40=\"\",\"\",O40)","v":65},{"$f":"IF(P40=\"\",\"\",P40)","v":55347.5},0,{"$f":"IF(S40=\"\",\"\",(K40*S40))","v":0},3,{"$f":"IF(U40=\"\",\"\",(K40*U40))","v":2554.5},"20:52:00","23:08:00",{"$f":"IF(M40=\"\",\"\",100*(M40/AC40/(AD40-AE40)))","v":50.209205020920557},{"$f":"IF(AA40=\"\",\"\",100-Y40-AA40)","v":10.484863401427475},{"$f":"IF(M40=\"\",\"\",100*(AF40+AG40)/(AD40-AE40))","v":39.305931577651968},100,60,2.2572222222222198,null,0.58055555555555505,0.30666666666666598,{"$f":"IF(AC40=\"\",\"\",AC40*(AD40-AE40))","v":135.4333333333332},"01/03/16 20:52:43","01/03/16 23:08:09",{"$f":"IF(AD40=\"\",\"\",ROUND(60*(AD40-SUM(AE40:AG40)),1))","v":82.2},{"$f":"IF(AK40=\"\",\"\",M40/AK40*60)","v":49.635036496350367},"00:00:00","00:34:50","00:18:24","00:53:14"]
["LA08600801","23",355.6,7.9,12.34,12.15,136919,"SAE 41B30H MOD.","U090","230",851.5,2.6179999999999999,53,{"$f":"IF(A41=\"\",\"\",M41*K41)","v":45129.5},53,{"$f":"IF(N41=\"\",\"\",IF(AND(T41=\"\",V41=\"\"),N41,IF(T41=\"\",N41-V41,IF(V41=\"\",N41-T41,(N41-T41-V41)))))","v":45129.5},{"$f":"IF(A41=\"\",\"\",Q40+O41)","v":118},{"$f":"IF(P41=\"\",\"\",R40+P41)","v":100477},0,{"$f":"IF(S41=\"\",\"\",(K41*S41))","v":0},0,{"$f":"IF(U41=\"\",\"\",(K41*U41))","v":0},"23:08:00","00:00:00",{"$f":"IF(M41=\"\",\"\",100*(M41/AC41/(AD41-AE41)))","v":102.21793635486989},{"$f":"IF(AA41=\"\",\"\",100-Y41-AA41)","v":-2.2179363548698916},{"$f":"IF(M41=\"\",\"\",100*(AF41+AG41)/(AD41-AE41))","v":0},100,60,0.86416666666666597,null,null,null,{"$f":"IF(AC41=\"\",\"\",AC41*(AD41-AE41))","v":51.849999999999959},"01/03/16 23:08:09","02/03/16 00:00:00",{"$f":"IF(AD41=\"\",\"\",ROUND(60*(AD41-SUM(AE41:AG41)),1))","v":51.9},{"$f":"IF(AK41=\"\",\"\",M41/AK41*60)","v":61.271676300578036},"00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"",{"$f":"IF(A42=\"\",\"\",Q41+O42)","v":""},{"$f":"IF(P42=\"\",\"\",R41+P42)","v":""},null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","",{"$f":"AE71/24","v":"00:00:00"},{"$f":"AF71/24","v":"00:00:00"},{"$f":"AG71/24","v":"00:00:00"},"00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,"","","",null,"",null,"",null,null,"","","",null,null,null,null,null,null,"",null,null,"","","00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"00:00:00","00:00:00","00:00:00","00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"00:00:00","00:00:00","00:00:00","00:00:00"]

{"sheet":"Boletim Parada","index":2,"n_rows":48,"n_cols":20,"rows_kept":48,"cut":false,"hidden":false,"merged":[[4,11,4,17],[4,18,5,18],[4,19,5,19],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,4,10],[2,18,2,19],[3,1,3,3],[3,4,3,6],[3,10,3,12],[3,13,3,14],[3,15,3,16],[3,18,3,19],[2,1,2,3],[2,4,2,6],[2,10,2,12],[2,13,2,14],[2,15,2,16],[2,17,3,17],[0,0,0,5],[0,6,0,17],[0,18,0,19],[1,1,1,3],[1,4,1,6],[1,7,1,9],[1,10,1,12],[1,13,1,14],[1,15,1,16],[1,18,1,19]]}
[null,null,null,null,null,null,"RELATÓRIO DE PARADAS E INTERRUPÇÕES",null,null,null,null,null,null,null,null,null,null,null,"Laminador - 100%"]
[24,"INTER. MECÂNICA",null,null,"INTER. ELÉTRICA",null,null,"INTER. OPERAÇÃO",null,null,"INTER. SET UP",null,null,"INTER. OUTROS",null,"TOTAL INTER.",null,"PARADAS","01/03/2016 a 02/03/2016"]
["h",{"$f":"SUMIF($H:$H,200,$D:$D)+SUMIF($H:$H,240,$D:$D)+SUMIF($H:$H,260,$D:$D)","v":0},null,null,{"$f":"SUMIF($H:$H,300,$D:$D)+SUMIF($H:$H,360,$D:$D)+SUMIF($H:$H,380,$D:$D)","v":8.2638888888888873E-2},null,null,null,{"$f":"SUMIF($H:$H,700,$D:$D)+SUMIF($H:$H,800,$D:$D)","v":3.8518518518518396E-2},null,{"$f":"SUMIF($F:$F,3,$D:$D)","v":0.21973379629629625},null,null,{"$f":"P3-B3-E3-I3-K3+1/24/60/60/100","v":1.1574074074074073E-7},null,{"$f":"SUMIF($F:$F,\"002\",$D:$D)+SUMIF($F:$F,\"003\",$D:$D)","v":0.34089120370370352},null,{"$f":"24*SUMIF($F:$F,\"001\",$D:$D)","v":6.8927777777777779},"RESPONSÁVEL"]
["%",{"$f":"100*24*B3/($A$2-$R$3)","v":0},null,null,{"$f":"100*24*E3/($A$2-$R$3)","v":11.593543987269831},null,null,null,{"$f":"100*24*I3/($A$2-$R$3)","v":5.4038255447666499},null,{"$f":"100*24*K3/($A$2-$R$3)","v":30.826811288279796},null,null,{"$f":"100*24*N3/($A$2-$R$3)","v":1.6237456564803685E-5},null,{"$f":"100*24*P3/($A$2-$R$3)","v":47.824180820316279}]
["Data","Início","Fim","Duração","Turno","Causa da Interrupção",null,null,null,null,null,"Local de Instalação",null,null,null,null,null,null,"Observação","Ordem de serviço"]
[null,null,null,null,null,"Cód.","Tipo","Cód.","Motivo","Cód.","Defeito","Área","Cód.","Equipamento","Cód.","Conjunto","Cód.","Subconjunto"]
["01/03/16","00:10:26","00:20:27",6.9560185185185202E-3,{"$f":"IF(B7=\"\",\"\",TRUNC(24*B7/8+1))","v":1},1,"PARADA PROGRAMADA",100,"PROGRAMADA","118","TURNO NAO ESCALADO","LAU",null,null,null,null,null,null," "]
["01/03/16","01:13:03","07:56:36",0.28024305555555556,{"$f":"IF(B8=\"\",\"\",TRUNC(24*B8/8+1))","v":1},1,"PARADA PROGRAMADA",100,"PROGRAMADA","118","TURNO NAO ESCALADO","LAU",null,null,null,null,null,null," "]
["01/03/16","08:52:19","08:57:46",3.7847222222222032E-3,2,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","001","PONTA/MANDRIL                   (3min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null,"TROCA DE PAREDE DE 15.11 PARA 12.70. "]
["01/03/16","09:16:47","09:48:50",2.2256944444444371E-2,2,3,"PARADA PARA PREPARACAO",906,"TROCA DE BITOLA","002","BIELA. PONTA/MANDRIL            (16min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null,"TROCA DE PARADE E BIELA DO LAMINADOR SWW E LAMINADOR 3. "]
["01/03/16","09:50:02","09:55:56",4.0972222222221966E-3,2,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","006","CONTROLANDO 1a PEÇA IMS (3 min)","LAU",40,"LAMINADOR DE LUPAS 3",450,"LAMINADOR 3 - MAQUINA",null,null,"AGUARDANDO A PRIMEIRA PEÇA PASSAR NO IMS. "]
["01/03/16","11:12:26","11:17:52",3.7731481481481088E-3,2,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","001","PONTA/MANDRIL                   (3min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null,"tTROCA DE PAREDE DE 20.24 PARA 21.44."]
["01/03/16","11:30:18","11:50:56",1.4328703703703649E-2,2,2,"PARADA NAO PROGRAMADA",800,"INTERRUPCAO DE PRODUCAO",null,null,"LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null,"RETIRAR LUPA COMPRIDA NA SAIDA DO SWW APÓS DEVERGENCIA DE INFORMAÇÃO ENTRE FOLHA PI E MTS. "]
["01/03/16","11:50:56","13:49:56",8.2638888888888873E-2,2,2,"PARADA NAO PROGRAMADA",300,"ELETRICA","332","FALTA DE FASE","LAU",30,"LAMINADOR DE BLOCOS SWW",250,"LAMINADOR SWW - SAIDA",530,"REMOVEDOR","AJUSTAR ATUADOR DO SENSOR DO REMOVEDOR DE SAIDA DEVIDO COLISÃO ENTRA  BIELA E O 1º BRAÇO DO REMOVEDOR.",104660125]
["01/03/16","13:51:39","13:56:51",3.6111111111111205E-3,2,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","006","CONTROLANDO 1a PEÇA IMS (3 min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null,"AGUARDANDO A PRIMEIRA PEÇA PASSAR NO IMS APÓS PARADA MECÂNICA. "]
["01/03/16","14:08:44","14:15:25",4.6412037037036891E-3,2,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","001","PONTA/MANDRIL                   (3min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null,"TROCA DE PAREDE DE 21.44 PARA  25.40."]
["01/03/16","14:25:32","14:29:10",2.5231481481480245E-3,2,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","006","CONTROLANDO 1a PEÇA IMS (3 min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null,"AGUARDANDO A PRIMEIRA PEÇA PASSAR NO IMS."]
["01/03/16","14:30:53","14:35:51",3.4490740740741321E-3,2,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","001","PONTA/MANDRIL                   (3min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null,"TROCA DE PAREDE DE 25.40 PARA 31.75. "]
["01/03/16","14:35:51","14:39:51",2.7777777777777679E-3,2,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","006","CONTROLANDO 1a PEÇA IMS (3 min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null,"AGUARDANDO A PRIMEIRA PEÇA PASSAR NO IMS."]
["01/03/16","14:41:34","14:47:35",4.1782407407408018E-3,2,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","001","PONTA/MANDRIL                   (3min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null,"TROCA DE PAREDE DE 31.75 PARA 36.50. "]
["01/03/16","14:50:56","14:56:04",3.564814814814854E-3,2,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","006","CONTROLANDO 1a PEÇA IMS (3 min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null,"AGUARDANDO A PRIMEIRA PEÇA PASSAR NO IMS. "]
["01/03/16","14:57:47","15:04:45",4.8379629629630161E-3,2,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","006","CONTROLANDO 1a PEÇA IMS (3 min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null,"AGUARDANDO A SEGUNDA PEÇA PASSAR NO IMS. "]
["01/03/16","15:28:50","15:36:45",5.4976851851851194E-3,2,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","001","PONTA/MANDRIL                   (3min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null,"TROCA DE PAREDE DE 36.50 PARA 30.00. "]
["01/03/16","15:38:34","15:44:19",3.9930555555556246E-3,2,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","006","CONTROLANDO 1a PEÇA IMS (3 min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null,"AGUARDANDO A SEGUNDA PEÇA PASSAR NO IMS.  "]
["01/03/16","16:04:21","16:07:30",2.1874999999998979E-3,3,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","001","PONTA/MANDRIL                   (3min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null," DE 30.00 X 36.50"]
["01/03/16","16:09:19","16:12:33",2.2453703703705363E-3,3,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","006","CONTROLANDO 1a PEÇA IMS (3 min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null," CONTROLAR PRIMEIRA PEÇA DA PARAEDE 36.50 NO IMS"]
["01/03/16","16:19:39","19:11:53",0.11960648148148145,3,3,"PARADA PARA PREPARACAO",908,"TROCA DE CALIBRE","010","CIL.SWW.LAM.PERIF.(PROG.PLP)  (130 min)","LAU",40,"LAMINADOR DE LUPAS 3",450,"LAMINADOR 3 - MAQUINA",null,null,"DE 3.270 PARA 1350. "]
["01/03/16","19:18:50","19:25:16",4.4675925925924398E-3,{"$f":"IF(B28=\"\",\"\",TRUNC(24*B28/8+1))","v":3},3,"PARADA PARA PREPARACAO",908,"TROCA DE CALIBRE","016","CONTROLANDO 1a PEÇA IMS (3 min)","LAU",40,"LAMINADOR DE LUPAS 3",450,"LAMINADOR 3 - MAQUINA",null,null,"CONTROLANDO 1ª PEÇA PASSAR PELO IMS APÓS TROCAR CALIBRE."]
["01/03/16","19:34:53","19:38:53",2.7777777777777679E-3,{"$f":"IF(B29=\"\",\"\",TRUNC(24*B29/8+1))","v":3},3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","001","PONTA/MANDRIL                   (3min)","LAU",30,"LAMINADOR DE BLOCOS SWW",240,"LAMINADOR SWW - MAQUINA",null,null,"DE 9.50 PARA 9.52. "]
["01/03/16","20:16:51","20:20:43",2.6851851851852349E-3,3,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","001","PONTA/MANDRIL                   (3min)","LAU",40,"LAMINADOR DE LUPAS 3",450,"LAMINADOR 3 - MAQUINA",null,null," DE 9.50 X 7.90"]
["01/03/16","21:09:09","21:27:33",1.2777777777777888E-2,3,3,"PARADA PARA PREPARACAO",904,"TROCA DE PAREDE","007","EQUALIZAÇÃO DE TEMPERATURA     (20 MINS)","LAU",70,"FORNO NASSHEUER",730,"FORNO NASSHEUER - AQUECIMENTO",null,null," FAZER VAGAS NO FORNO NASSHEUER PARA EQUALIZAR TEMPERATURA PARA ENFORNAMENTO DO GARRAFA 355.6 X 7.90    41B30"]
["01/03/16","21:46:55","21:50:01",2.1527777777776702E-3,3,2,"PARADA NAO PROGRAMADA",800,"INTERRUPCAO DE PRODUCAO",null,null,"LAU",55,"LAMINADOR ALISADOR - REELER II",30,"LAMINADOR ALISADOR REELER II - MAQUINA",null,null," REELER 2 PARADO PARA CORRIGIR AMASSAMENTO NO MATERIAL  E EXCESSO DE TUBOS NO REELER 1."]
["01/03/16","22:17:05","22:32:43",1.0856481481481439E-2,3,2,"PARADA NAO PROGRAMADA",800,"INTERRUPCAO DE PRODUCAO",null,null,"LAU",40,"LAMINADOR DE LUPAS 3",430,"LAMINADOR 3 - ENTRADA",null,null,"RETIRAR SUCATA NO LAMINADOR 3 COM AUXILIO DA PONTE 10 DEVIDO O TUBO TER RASGADO NO MANDRIL DE 2º PASSE. "]
["01/03/16","22:33:48","22:49:54",1.1180555555555638E-2,3,2,"PARADA NAO PROGRAMADA",800,"INTERRUPCAO DE PRODUCAO",null,null,"LAU",40,"LAMINADOR DE LUPAS 3",430,"LAMINADOR 3 - ENTRADA",null,null," RETIRAR SUCATA NO LAMINADOR 3 COM AUXILIO DA PONTE 10 DEVIDO O TUBO TER  AGARRADO NO MANDRIL DE 1º PASSE."]
[null,null,null,"",""]
[null,null,null,"",""]
[null,null,null,"",""]
[null,null,null,"",""]
[null,null,null,"",""]
[null,null,null,"",""]
[null,null,null,"",""]
[null,null,null,"",""]
[null,null,null,"",""]
[null,null,null,"",""]
[null,null,null,"",""]
[null,null,null,"",""]
[null,null,null,"",""]
[null,null,null,"",""]